
Skillet Name – Activate PANOS Licenses Offline

# 

# 

# Brief Description

This skillet provides the step-by-step licenses activation for PANOS when the device could not connect to Internet.

# Target Audience

SEs, Partners, Customers.

# Skillet Details

**Authoring Group**: SecOps

**Documentation**: documentation will be provided soon

**Github Location**: https://github.com/zhiyhappy/ezhi-activate-license-offline.git

**PAN-OS Supported**: Tested on PAN-OS 8.0 & above

**Cloud Provider(s) Supported**: All

**Type of Skillet**: XML

**Purpose**: Config

**Status**: draft

# Detail Description

Provide a detailed description of what the Skillet does, what the value is and a high level overview of how it works. Should be a combination of text and graphics, depicting the overall configuration of the skillet. Think in the following format:

* 3 sentences on what it does
  + The skillet provides step-by-step licenses activation for PANOS when the device could not connect to Internet
  + The skillet provides GUI for users to activate license with auth code
  + The skillet also helps users to check the PANOS license information and auth-code usage information
* what is the value to the target audience
  + The skillet helps the target audiences to activate the PANOS device which could not connect to Internet via one GUI step-by-step, they don’t need to work on the whole process manually.
* general overview on how to deploy, or execute demo
  + Step 1, get PANOS device API Key
  + Step 2, get PANOS device CPUID & UUID via the API Key
  + Step 3, activate license with CPUID & UUID and Auth-code in Palo Alto Networks licensing system, get the license key, and then manually install the license key into PANOS device
  + Step 4, check the PANOS device license information
  + Step 5, check the auth-code usage from Palo Alto Networks licensing system
* expected outcome
  + After activate the auth-code with CPUID & UUID in Palo Alto Networks licensing system, user still need to copy the license keys and install the keys into the PANOS device.